This video shows a loop closure in outdoor SLAM. The figure on the left shows images obtained from a high-resolution camera mounted at the top of a modified car. The squares indicate recognised landmarks with crosses representing the projection of laser points. The right figure shows the map with the estimated trajectory (blue), GPS estimation (green) and landmark pose estimation (blue points). Note that the map is updated when the loop closure is detected.
