The video shows a typical situation where sICP and sIDC algorithms get trapped by a local minimum. This trapping situation 
is due to the large initial error and the low angular resolution of sonar sensors. By using probabilistic sonar and odometry
models, our scan matching proposal, the spIC, is not trapped by the local minima. This fact is shown in the video.