a: Description: 
  This video shows that a fish-like robot actuated by an electrostatic film motor is capable of swimming in dielectric liquid (i.e., Fluorinert FC-77) by using open-loop control strategies. The fish-like robot cruises with a general speed of approximately 0.018 m/s. Moreover, it can accomplish better fish-like maneuverability, for example turning and diving motion. 


b: Player Information: 
  This video is a mpeg1 format file. It can be played by Windows Media Player. 


c: Contact Information:
  heroeiyou@ieee.org

Attachment filename: 0231_VI.mpg (4990980 Bytes)