a. Description: 
This video shows controlled motion of the 3-DOF Gantry-Tau parallel
kinematic manipulator initially prototyped at the University of
Queensland, Australia. The robot holds a spindle and is intended
for machining applications.

b. Player Information:
Windows Media Player 9

c. Contact Information:
Prof. Geir Hovland
Agder University College
Serviceboks 509
N-4898 Grimstad, Norway
Email: geir_hovland@ieee.org



Attachment filename: 0424_VI.mpg (4998956 Bytes)