This video shows controlled motion of the 3-DOF Gantry-Tau parallel
kinematic manipulator initially prototyped at the University of
Queensland, Australia. The robot holds a spindle and is intended
for machining applications.
