This video presents the simulation results of a new visual control approach based on homography with nonholonomic motion constraints.
The control law is designed by the input-output linearization of the system using elements of the homography as output.
The simulations show the trajectories followed by the robot starting from three different initial positions.