This video presents the simulation results of a switched homography-based visual control for differential drive vehicles.
The control drives the robot along optimal paths taking into account the field-of-view constraints of the vision system.
The optimal paths consist of straight lines and curves that saturate the sensor viewing angle.
The video shows the trajectories followed by the robot in three different simulations with straight line and T-curve paths.