This video demonstrates the performance of the bending laser manipulator for intrauterine surgery ( 2.4mm in diameter, 2 DOF of bending).  The manipulator during a positioning test, in vitro test and in vivo test were shown.