a. Description: This video demonstrates the performance of the bending laser manipulator for intrauterine surgery ( 2.4mm in diameter, 2 DOF of bending).  The manipulator during a positioning test, in vitro test and in vivo test were shown.
b. Player Information: This file is mpeg1 format (without audio due to the max file size restriction).
c. Contact Information: hkanako@suou.waseda.jp

Attachment filename: 0883_VI.mpg (5187168 Bytes)