This video shows a loop-closing real image sequence experiment that shows the impressive performance of 'inverse depth initialization' plus 'inverse depth to depth conversion' in 6 DoF SLAM with a single camera. The image sequence and a top view of the estimated map (with its covariance) are displayed. The image sequence was recorded with a hand-held wide-angle lens camera in a computer room.