This video shows the performance of the automatic relocalisation module for single-camera SLAM systems. The robustness to occulisions and rapid camera motions is demonstrated in an office environment. The module is able to run on live sequences of 33Hz and generally recovers within 1-2 frames.