The video shows the robot mounted tactile sensor plate while probing
two different objects. In the lower left corner you can see the
tactile image recorded from the sensor. 

File is in MP4 Format, 640x480 24bpp  25.000 fps 

Selected video codec: [ffodivx] vfm: ffmpeg (FFmpeg MPEG-4)

Author contact information: 
Matthias Schoepfer
Bielefeld University, Germany
mschoepf@techfak.uni-bielefeld.de
Phone: +49 521 106-2941

Attachment filename: 1512_VI.mp4 (3440640 Bytes)