The video demonstrates the capability of the powered tethered prosthetic device in level walking on a treadmill at a speed of 0.675 m/s (1.5 mph) with starting and stopping utilizizing the finite-state impedance based controller outlined in the paper.