The motion of a voltage-induction-type two-four-phase electrostatic film motor, 
which requires no electric wiring to the slider, is shown in the movie.
In the former part of the movie, wired-type of the motor with same driving-electrode configuration demonstrates the performance 
of the electrode configuration, which is proposed in this paper.
