-----------------------------------
Desciption:
-----------------------------------
This clip shows the different results when a user is tying an overhand knot with different models mentioned in this paper. Two unknotting procedures of model four are also shown in this clip.
1. Model one ( red ) has only linear spring and linear damper
2. Model two ( yellow ) is based on model one + torsional spring
3. Model three ( green ) is based on model two + torsional damper
4. Model four ( blue ) is based on model three + swivel damper
5. Model five (pink) has the same compnents as model four, but the linear spring force is computued quadrtically on the difference between its current length and the rest length.

------------------------------------
Player Information:
------------------------------------

Length: 54 seconds
Dimention: 640 X 480
Format: MPEG-4

It needs QuickTime Player v7.1.3 or later
----------------------------------
Contact Information:
----------------------------------
Name: Hans Fuhan Shi
E-mail: fuhans@ensc.sfu.ca


Attachment filename: 1292_VI.mp4 (4527357 Bytes)